This archive contains the All_EMU_plugin for KARG Fortis STB's
( Optibox Koala, Anaconda, Raptor and Gekko ).

Oscam KARG ( oscam ) - webif defaults are port=8888 and
 user/passwd=karg/karg , you must edit oscam.server in 
/var/keys  for CCcam "C:" or "N:" lines , in order to
"read" cards you can consult the included oscam.server for
some examples

Mgcamd ( mgcamd.sh4 ) - 1.38 - you must edit in /var/keys/ the
cccam.list file ( for CCcam C: lines ) or newcamd.list file 
( for NewCS N: lines or CSP lines ) Pay attention to boxtype 
usage in /var/keys/mg_cfg ...

Mcas  - is the multicas card reader and softcam emu in order to
 "read" cards you must disable conax reader from menu , stop 
Oscamd or MgCamd ( if active ) MCas is a local EMU based on 
keydata.tnp key file , local crdserver and homesharing crdserver
in conjunction with Mclient. Coconut is the Biss keys EMU and
biss keys table editor.


Note 1 : installing this plugin you overide previous content of
/var/keys by consequence you must backup the previous  content 
if needed ( oscam.server)

Note 2 : we strongly recommend to use a Linux editor (UltraEdit)
to edit the config files ! elsewhere Oscam will not understand
your files ! anyway you must edit only octagon.server ! the rest
... is a good ideea to remain unchanged !!!

Note 3 : before installing this release , we strongly recommend ,
to do a folder cleanup using FTP client ... clean /var/bin !!!

