  relook400s software release

  released version  : 2.9.alpha
  released date     : Thu Jul 13 15:07:57 KST 2006


1.version
    - boot loader
      U-Boot 1.1.1(Jul 13 2006 - 14:46:17)
    - application
      2.9.
    - database
      1.15


usb_db.img
via usb cable, it formats the database. It requires
rescanning of channels.

usb_kernel_root.img
via usb cable, it updates linux kernel and applications only.


=======================================================
 How to download
=======================================================
1.Check your current program version first: Main menu-->About-->system info -->program version.

2.1 : If the program version is older than it's newly released, kernel_root.img has to be downloaded.

2.2: If the DB version is older than it's newly released, db.img has to be replaced.

=======================================================
 2.9 Changes
=======================================================
[Function added]
-Mount manager developed by relookusers team has been added which allow users to share PC's certain directory. 

[Function added]
-Mutant200S only: file system protocol has been added which allows users to share files such as samba,nfs,cifs.

[bug fixed]
-Channel names appears with wrong/unusual letter due to error in encoding process , when channel scan is done.
  
[bug fixed] 
-Characters in EPG list contains wrong characters and symbols on  particular TPs.  

[bug fixed]
-When booted, we have a feedback that tv screen sometimes shows TEST pattern without getting outputs for tv screen properly.
 (This bug is fixed in this new uboot.img  However, this is for the users who experience this problem. If you are not the case, we 
do not recommend to upgrade this new bootloader). 
       
[Improved]
-Mutant 200S : Database part space is increased.
[Notice] This increase of Database space in this version is related with database part, so db.img have to be downloaded this time.
(Be careful that you will loose all your current data if download this db.img, so Back-up all data first to your PC by PCEditor)

[Improved]
-Since cursor color is same as character¡¯s in multifeed window,those two are not distinguishable. Now it is improved by changing colors.
     
[Improved]
-relook 400S only: multifeed window can be open directly by pressing multifeed button. 

[Function added]
-Short cut function is added in channel list when channel is sorted.  
For example, When sorted from A-Z, pressing #5 on RCU will lead you to channels stating Alphabet J, 
pressing one more time the same button (#5) consecutively, you will be at channels starting alphabet K, 
three times(#5) consecutively to channels starting alphabet L.

[Improved]
- Several known bugs fixed.

-------------------------
* Known bugs
    - relook 400S : Sometimes get PANIC when zapping between the channels by using 'recall' function while recording two channels simutaneously that has teletext information.
    - mutant 200S : Sometimes get error message like "no more disc space" while Network upgrading and fail to download.  If you get this trouble, please use Flashtool.
-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------     


[Warning/Important Notice]
 
1. Database(db.img) file download : 
 To use this 2.9 version software, database (db.img) is required to be downloaded, 
Therefore you have to Back-Up channel/favorite data first to your PC by using PCEditor program. Otherwise you will loose all data and have to rescan&edit channels again.
 
2. Bootloader(uboot.img) file download : 
 If you see a problem with TV screen after booting, download this new uboot.img.
 While uboot.img downloading, you should be very careful.  
 If there is any Power off or some failure while downloading, it can cause serious damage on receiver. 
 So, be careful always when u-boot downloading procedure!!!
 * uboot image can not be upgraded via network(LAN), it has to be flashed with Flashtool either USB(relook 400S) or Serial port(mutant 200S).
