# CCcam team uvadi CCcam v1.6.2
#
# Special greets go to Dale Cooper, the RuDream and ofcourse HDLteam
#
# For system without new enigma socket.... capmtserver is your friend ;-)
#

######################################################################
# friends                                                            #
######################################################################
# syntax for to add a friend user to CCcam with the max up hops limit (default = 5)
# sharing of emus (default = 1), allow emm (default = 1), and optional
# downshare limits per share (default = no limits) and optional
# downshare limits per share based on caid:id:sid
# and optional timeslots in which share is valid (to block channels on box of children after 19:00 for instance)
# if no timeslot is defined 24 hrs a day is used
# emus are shared only one level down, even if no limits given
#
# max username length 20
# password length 'unlimited'
#
#F: <username> <password> <uphops> <shareemus> <allowemm> ( { caid:id(:downhops), caid:id(:downhops), ... } { caid:id:sid, caid:id:sid, ... } { begintime-endtime, ... } )
#
# example:
#
# F: user1 pass1
#
# user1 gets all our shares at max 5 hops from us
# (our local cards + max five hops away). He can share down to his own
# clients. He also receive emu shares (if he has 'yes' behind his C: entry),
# and is allowed to send us emm.
#
# F: user2 pass2 0 1 0 { 0100:000080, 0622:000000:1, 0500:000000:2 }
#
# user2 gets only our local cards but no 0100:000080.
# and our 0622:000000 cards only for himself (1 hop down),
# and 0500 cards for himself plus one additional hop down.
# He also gets our emus, and is NOT allowed to send us emm (updates).
#
# F: user3 pass3 5 0 1 { 0:0:3, 0100:000080:1 }
#
# user3 gets all cards at a maximum of 5 hops away from us,
# and get's to share them down two further levels beyond his own level.
# But he is not allowed to share 0100:000080 down to other users.
# He gets no emus from us, and he is allowed to send us emm.
#
# F: user4 pass4 5 0 1 { 0:0:3, 0100:000080:1 } { 0100:000080:15df }
#
# user4 gets all cards at a maximum of 5 hops away from us,
# and get's to share them down two further levels beyond his own level.
# But he is not allowed to share 0100:000080 down to other users.
# He gets no emus from us, and he is allowed to send us emm.
# He is also not allowed to view channel 0100:000080:15df
#
# F: user4 pass4 5 0 1 { } { } { 12:00-17:00, 19:00-20:00 }
#
# user4 gets all cards at a maximum of 5 hops away from us,
# and get's to share them down two further levels beyond his own level.
# the share is only valid between 12:00 and 17:00 and between 19:00 and 20:00
# outside these hours the share will not give cw's to the client


######################################################################
# connections                                                        #
######################################################################
# syntax for to add a client connection to other CCcam
# add yes on end to use friends emus (non public private key/emu,etc...),
# but only works when corresponding F line on server has '1' for <shareemus>
# optional limits just like F line, but for incoming shares (ignore shares more than 'uphops' away)
#
#C: <hostname> <port> <username> <password> <wantemus> ( { caid:id(:uphops), caid:id(:uphops), ... } )
#
#note: if {} limits are added, <wantemus> cannot be omitted. Use either yes or no.
#
# example:
#
# C: someserver.somedomain 12000 user1 pass1
# C: 192.168.1.2 12000 user2 pass2
# connects to CCcam without use of friends emus
#
# C: 192.168.1.2 12000 user3 pass3 yes
# connects to CCcam, and receives friends emus also.


# syntax for to add newcamd server connection
#
#N: <ip> <port> <username> <pass> <des(14byte)> <nr_of_hops_away (default: 1)> <stealth mode (default: 0)>
#
# example:
#
# N: 127.0.0.1 10000 dummy dummy 01 02 03 04 05 06 07 08 09 10 11 12 13 14
#
# add a newcamd card, give it an offset of 2 hops, in the share list
#
# N: 127.0.0.1 10000 dummy dummy 01 02 03 04 05 06 07 08 09 10 11 12 13 14 2
#
# stealthy login on newcamd server:
#
# N: 127.0.0.1 10000 dummy dummy 01 02 03 04 05 06 07 08 09 10 11 12 13 14 1 1
#
# stealth modes: 0 = disabled, 1 = mgcamd new, 2 = mgcamd old, 3 = evocamd, 4 = generic


# syntax for to add radegast server connection
#
#R: <ip> <port> <ca4> <id6> <nr_of_hops_away (default: 1)>
#
# example:
#
# R: 127.0.0.1 678 0100 000080


# syntax for to add camd3 connection
#
#L: <ip> <port> <username> <pass> <ca4> <id6> <nr_of_hops_away (default: 1)>
#
# example:
#
# L: 127.0.0.1 567 dummy dummy 0100 000080


######################################################################
# Other config settings                                              #
######################################################################
# server shall listen on this port pro incoming connections
# default port is 12000, disable server with parm -s or set port 0
#
#SERVER LISTEN PORT : 12000

# server can give some info about server and client connections
# and cardinfo using telnet or webbrowser.
#
# Switch on/off access to info
# default is yes
#
#ALLOW TELNETINFO: no
#ALLOW WEBINFO: no

# The webinfo service can be protected with a username and password.
# This is switched off by default
#
#WEBINFO USERNAME : <username>
#WEBINFO PASSWORD : <password>

# The telnetinfo service can be protected with a username and password.
# This is switched off by default
#
#TELNETINFO USERNAME : <username>
#TELNETINFO PASSWORD : <password>

# default port for telnet is 16000
# default port for web is 16001
# supported commands:
#        info
#        activeclients
#        clients
#        servers
#        shares
#        providers
#        entitlements
# example use:
#     echo servers | telnet localhost 16000
#     go with your browser to http://ip_CCcam_server:16001
#
#TELNETINFO LISTEN PORT : 16000
#WEBINFO LISTEN PORT : 16001

# time in seconds to keep On Screen Display active.
# default is 0 (turned off)
#
#ZAP OSD TIME : 3

# username used to show popup (default : root)
#OSD USERNAME : root

# password used to show popup (default : dreambox)
#OSD PASSWORD : dreambox

# port used to show popup (default : 80)
#OSD PORT : 80

# Serial path to phoenix reader. Add as many as you have attached too your system
# default is none
# optionally add readertype : phoenix,mouse,uniprog
# (when non readertype given defaults to uniprog (e.g. for mastera))
#
#       Phoenix Reader Path : <device> <type>
#
# example
#
#PHOENIX READER PATH : /dev/tts/0


# if timing should be shown in OSD and debug output
# default is no (turned off)
#
#SHOW TIMING : yes

# enables mini OSD which shows server(type), cardreader, keys or fta only
# default is no (turned off)
#
#MINI OSD : yes

# turns debugging on and off
# default is no (turned off)
#
#DEBUG : yes


# should CCcam try to read and parse newcamd.conf for server connections
# default is no (turned off)
#
#NEWCAMD CONF : yes


# configure what EMM blocker you want. Add as many as readers you have attached
# default is blocking nothing
#
# B: /dev/sci0 01
#       00 - nothing
#       01 - sa blocked
#       02 - ua blocked
#       04 - ga blocked
#       and sum of for combinations
#
#examples
#
#B: /dev/tts/0 07
#B: /dev/sci0 01

# disable all local EMM readers
# saves lots of CPU, but you won't get any updates anymore
# (unless you get updates from your clients)
#
# default: no
#
#DISABLE EMM : yes

# with this setting you can
# allow a client on two hops away
# to send the updates to the cardserver
#
# default : no
#
#EXTRA EMM LEVEL : yes

# overrule the nds boxkey (4 byte hex)
#
# BOXKEY: <device> <byte1> <byte2> <byte3> <byte4>
#
#example
#
#BOXKEY: /dev/sci0 00 11 22 33

# set card pin
# * please be very careful with this option as you could lock your card *
#
# PIN: <device> <pin>
#
#example
#
#PIN: /dev/sci0 9999

# overrule the irdeto camkey (8 byte hex), default 11 22 33 44 55 66 77 88
#
# CAMKEY: <device> <byte1> <byte2> <byte3> <byte4> <byte5> <byte6> <byte7> <byte8>
#
#example
#
#CAMKEY: /dev/sci0 11 22 33 44 55 66 77 88

# overrule the irdeto camdata (64 byte hex)
# trailing zero bytes can be omitted
# default for unknown ASC's is 11 22 33 44 55 66 77 88 00 00 .. 00, known ASC's have other defaults
#
# CAMDATA: <device> <byte1> <byte2> <byte3> <byte4> <byte5> <byte6> ... <byte64>
#
#example, when only the first 15 camdata bytes are nonzero
#
#CAMDATA: /dev/sci0 11 22 33 44 55 66 77 88 99 aa bb cc dd ee ff

# custom add id's for BEEF patched cards
#
# BEEF ID: <ident1> <ident2> <ident3> <ident4> <ident5> <ident6> <ident7> <ident8> <device>
#
#example
#
#BEEF ID: 4101 0 0 0 0 0 0 0 /dev/sci0

# what Softcam.Key should CCcam try to read
# defaults to /var/keys/SoftCam.Key
#
#SOFTKEY FILE : /var/keys/SoftCam.Key


# what AutoRoll.Key should CCcam try to read
# defaults to /var/keys/AutoRoll.Key
#
#AUTOROLL FILE : /var/keys/AutoRoll.Key


# what constant.cw should CCcam try to read
# defaults to /var/keys/constant.cw
# file content can be like
#
# ca4:id6:sid4:pmtpid4:ecmpid4:key16(01 02 03...)
#
#STATIC CW FILE : /var/keys/constant.cw


# in this file you can configure what CAIDs CCcam should prefer or ignore
# defaults to /var/etc/CCcam.prio
# file content can have ignores (I) and prio lists (P)
#
# note 1: I line affects both for ecm and emm (receive no emm on ignored systems)
# P line only affects ecm choice (emm still received for all available systems, not just the priority system)
#
# note 2: ident 0 means 'all idents'. So 'caid:0' is the same as 'caid'.
#
# note 3: for some systems (e.g. nagra (caid 18xx)), the ident is not known at the time the
# prio lists are checked. In that case, matching is done on caid only, even if the P line
# defines nonzero idents. So for example '1801:401' behaves the same as '1801' in a P line
# I lines work differently, they are checked two times, once before ecm or emm is received, again
# after ecm or emm are received (and nagra ident should be known)
# P lines are only checked once, before ecm received.
#
# note 4: if a P line contains caid:ident pairs which are not available for the current
# channel, that P line is not used for that channel.
# Example, channel has systems 626, 1801:401 then P line with "1801,100:96,626" is ignored by that channel,
# because channel doesn't have 100:96.
# But P line with "1801" works, and also "626,1801" will work for channel
#
# note 5: P lines are parsed in the order in which they are found in the prio file.
# Only the first matching P line is used
#
# situation 1: ignore allways this caid, all idents, on all channels
# I: caid
#
# situation 2: ignore allways this caid/ident pair
# I: caid:ident
#
# situation 3: ignore this caid/ident pair, on channel 'sid'
# I: caid:ident:sid
#
# situation 4: when both caid1 and caid2 exist for a channel, prefer caid1 over caid2
# P: caid1, caid2
#
# situation 5: when caid1:ident1 till caidN:identN exist for a channel, use them in order of this list.
# P: caid1:ident1, caid2:ident2, .., caidN:identN
#
# situation 6: when caid1:ident1 till caidN:identN exist for channel 'sid', use them in order of this list.
# Sid on first caid/ident pair identifies sid for which list is used. All other sids ignore this list.
# P: caid1:ident1:sid, caid2:ident2, .., caidN:identN
#
#CAID PRIO FILE : /var/etc/CCcam.prio


# write wrong logins to file
# defaults is off
#
#LOG WARNINGS : /tmp/warnings.txt

# global setting for stealthy login to newcamd/newcs server, N line can overrule
# stealth modes: 0 = disabled, 1 = mgcamd new, 2 = mgcamd old, 3 = evocamd, 4 = generic
# default: 0
#
#NEWCAMD STEALTH : 0

# load balancing between identical cards, list device names of card readers containing identical cards,
# optionally followed by a list of service id's which are to be excluded from loadbalancing
#
# LOADBALANCE : <device1> <device2> .. <devicen> { <exceptsid1>, <exceptsid2> .. , <exceptsidn> }
#
# multiple loadbalance groups can be configured, by adding multiple lines
# warning: restart is required, when loadbalance group config changes
#
#example 1: load balance requests for three identical cards
#
# LOADBALANCE : /dev/ttyS0 /dev/ttyS1 /dev/ttyS2
#
#example 2: load balance requests for two almost identical cards, sid 0df3 and 0de1 are only available
#on one of the cards, so requests for these sids shouldn't be loadbalanced
#
# LOADBALANCE : /dev/ttyS5 /dev/ttyS6 { 0df3,0de1 }

# in version 1.2.1 and lower there was a problem which could lead to disconnecting clients
# in version 1.4.0 network load was significantly reduced
# in order to take advantage of these fixes, all clients should upgrade
# with this setting you can force that clients at least use a certain version otherwise they are denied when logging in
#
# default : accept all versions
#
#example 1: avoid disconnecting clients problem
#
#MINIMUM CLIENT VERSION : 1.3.0
#
#example 2: achieve network load decrease
#
#MINIMUM CLIENT VERSION : 1.4.0


# Irdeto smartcards: option to disable smart chid checking for irdeto smartcards.
# Default, only chids advertised by card are accepted.
# This avoids a lot of unwanted card traffic
#
# But if smartcard has hidden/unknown chids, all chids should be tried.
# In that case specify 'TRY ALL CHIDS' option for cardreader.
# Use with care, enabling option causes more card traffic.
# Only use setting when some channels don't work without it.
# note: if even this setting don't help decode all channels, try using
# commandline arg -l, to disable all self-learning features (warning: slower)
#
#TRY ALL CHIDS : <device>
#
#example: card in /dev/ttyUSB0 gets ecm for all possible chids, not
#just the chids it officially supports
#
#TRY ALL CHIDS : /dev/ttyUSB0
