CATone V2.7

File CRC: FD50D77B
File MD5: f0ad05913c1bef12720deb8c8f0da9a5

CATone V2.8
- Coming soon
- Fixed DCW and BISS key handling

History and changes
CATone V2.7
- 16 Cryptoworks providers added subtracting 48 bytes to keyspace.
- Pressing Epg in Ram editor allows to select 4 working modes:
	- both original Nagra - 5 providers and new Nagra - 17 providers (N-5  N-17)
	- Cryptowrks  (CR + N-5  CR + N-17)
- Cryptoworks CA system is directly accessed by grey key "mute"
- P+ and P- may now be used to cyclically switch Coding system
- Corrected edit mode in PMCT. Pressing OK allows to add a new raw to PMCT ram only if it is not
  already present otherwise it will be modified.
- in ECM-DW submenu is now possible to check fixed DCW adding them to pmct ram 
	in this format: CA CA KEY KEY KEY KEY KEY KEY KEY KEY
	example
									06 08  11  22  33  44  55  66  77  88
	to place 16 bytes simply edit twice.								
	

CATone V2.6
- Changed Nagra Irdeto Mode Detection.
 	One byte at offset is 0x208 is checked. 
 	If it is equal to 0x05 (5) then Bin File will be read as a traditional Bin File (N-5)
 	If it is 0x011 (17) then Bin is read as new type.(N-17)
 	All other values are forced to be 0x11 (N-17).
 	Pressing EPG allows to override automatic detection and to manually select desired mode  

CATone V2.5
- Fixed Bugs in nagra providers detection
- Added Enhanced Nagra Irdeto Mode to host 17 nagra providers (HOT>=7.1). 
  To select this mode press EPG while Ram Editor is ON. This setting is stored and automatically recalled.

CATone V2.4
- Not Public	

CATone V2.3
- Fixed small bugs
- Changed Teletext description in parser

CATone V2.2 
- Not Public

- 	Added Edit Mode in PMT parser. Just select blue tab and OK on the desired line, 
		and an item will be added at the end of PMCT
- 	Now it's possible to delete keys and providers. In ram editor just press three times ON/OFF (STDBY) button
  	on the desired item. A self-disappearing banner will confirm operation. 
  	Deleting a provider cause the deletion of all its keys.
- 	Adjusted some minor bugs (hope not to have added further ones)
-   scrolling on LCD
.....


CATone V2.1

- Key Edit select CA system by rcu colors;
- in case current channel is decripted by emu the editor should start showing actual provider
	and key in use marked in red (in Irdeto,Beta it only shows 1st Iredto provider);
- Provider name for known providers is shown;
- Fully implemented CAT and PMT parser. 3 views available : compact, full, hex data;
- views and preferences are now stored:
	-> possible to use different color schemes for 
		 a-start menu, about and help
		 b-key editor
		 c-parser
		 d-ecm-dw
	-> preferred parser view is stored for both CAT and PMT (may be different)
	-> at each calling CATone starts recalling last stored views.
	-> CATone preferences (and other things :) ) are resetted when reloading complete setting list.


CATone is free. Nothing may be modified. Neither FW nor Strings. 
This readme should accompany any CATone distribution.

Enjoy.

SuD

CATone v 2.0

- Not Public 


CATone v 1.4

- Not Public 


CATone v 1.3 

- corrected additional bugs 
- fully implemented AU fields editing 



CATone v 1.2

- Not Public 



CATone v 1.1 

- Corrected some bugs; 
- resizing to easily fit in 16/9 screens 


CATone v 1.0 

IT is still not complete and to improve it. 
known issues: 
- Not possible to edit PPUA, HMK,PMK, etc etc. for AU (TO do but the only one needed is Irdeto cause others are not AU) 
- Not possible to edit Conax Keys (I think nobady will have patience to write 128 bytes by hands) 
- PMT parser is missing (on going) 
- Problems on 16/9 screens or some clipping while editing keys in some 4/3 (I have to compoct keys).


Thanks to ToH for their precious work, and to Humax-Zone.net for the support.


CATone is free. Nothing may be modified. Neither FW nor Strings. 
This readme should accompany any CATone distribution.

Sturm und Drang.