incubusCamd, cam daemon.
---------------------------------------------------------------------------------

Available for processor types: sh4 (tested only on Cuberevo, Cuberevo mini with e2), sigma (azboxhd)

Use the e2 version on kathrein with enigma 2 on board, the other version (*.sh4) on ipbox 9000/900 with dgstation firmwares
Use the sigma version on azbox hd firmwares

Card client for protocols: cccam, gbox, newcamd 5.20, newcamd 5.25, radegast old, radegast new, aroureos

.conf and .prio files can be inserted in the /var/bin directory, or in /etc, or in /var/keys

----------------
History:

07/02/2009, V0.70
- added auto-reconnection on servers (if lost connection previously)
- fixed a bug that caused the lost of cws
- added multi-server support for cccam (you can connect as a client to more than one server, this is a beta try, seems almost stable but it could have many bugs)
- fixed nagra providers (nagra3 and nagra2) interpretation (now they should work on cccam protocol, but i've not tested it so please report if you find bugs)
- fixed biss over cccam protocol
- added possibility to get emu shared data by server on cccam protocol (see config file)
- added logs information from console and into file (see config file)
- changed a bit the config file

Consider this version as a BETA one, i don't think it's really stable as i can think.
GBOX protocol is not fully supported in this version, I will fix it in the next release.

04/01/2009, V0.55
- fixed some little bugs on DGStations api interface
- added multi descrambling support for DGStations HD original firmwares (PIP, timeshift, recording channels, second tuner support)
- added version sigma to be used with AzBox HD
I've been noticed about many peoples not able to view some channels, don't forget to edit your prio file. Editing that file will give you the ability to chose the right pid wich the cam should be select (if you will not edit it, the cam will use the first pid and then try to use other pids, but this will take much more time to be able to see something)

20/06/2008, V0.50, First public release
camd33 and camd35 is really much unstable so I think it's not yet ready for public, 
asap it will be ready i'll publish it ;)
This is the first release, you can't see any log on the console because 
I don't wanna people read infos that could put them on the strange way.
However logs on console are really good to know if bugs are the cause of your problem or 
simply if you are so noob to not be able to configure it correctly.

Read very well config files and don't say something you don't know.

This is not a fully working cam, some functions are not implemented/enabled because they are not ready for public and
I think people don't wanna functions that are working not really good as they expected!
(also this version is a beta version, but i wanted to put some hopes on people that believe a cam is better than othern one,
we have tested the cam on many decoders and we can say this cam is not bad at all also in beta and not full working mode :p)

So for the first release I choose to public only client side of the cam. :)

I want to thank raton_craquero for givin' me the possibility to know really a lot of things on how to use dvb_api and i have
to admit that i really like his config file structure and his log functions, so i decided to use them with his agreement :)
Thank you!

Regards, the IncubusCrew!
