Software update instructions for the DigiCorder HD S2X
==================================================

You can download a PDF file (requires Acrobat Reader) of the operating instructions for the DigiCorder HD S2X at:
http://www.technisat.de 


Installation:
First, copy the following files to a directory of your choice (e.g. C:\Technisat).

xxxxxxxxx.cpad
INFO.TXT
autoupdate
singleupdate


USB update instructions
====================

You need a commercially available USB flash stick to update the receiver using the USB interface. Format this USB flash stick with the "FAT32" file system. Now copy the software file "xxxxxxxxx.cpad" to the USB stick.


If you only want to perform a single update, also copy the "singleupdate" file to the USB flash stick.
If you wish to perform multiple updates with this USB flash stick, copy the "autoupdate" file to the USB flash stick instead.

Caution:
You should not have multiple PAD software files on the USB flash stick. The "autoupdate" and "singleupdate" files should also not be on the USB flash stick at the same time.

Now switch the receiver to standby mode and insert the USB flash stick in the USB port on the receiver. You can now turn on the receiver. After a few seconds, the message "USB Load" will appear on the display (followed by additional status messages) while the update is being performed.
When the message "USB Load done" or "Welcome" appears on the display, the update is complete. You can remove the USB stick.


If the USB update does not start, please repeat all of the steps or try using a different USB flash stick.


(c) TechniSat 2009
Subject to changes
