#Example configuration file for sbox cardclient server

# [slot0]	# slot to connect
# user=edk	# user
# pass=edk	# password
# au=1		# au on/off


# [slot1]	# slot to connect
# user=edk2	# user
# pass=edk2	# password
# au=0		# au on/off

