# debug messages level

# EMM messages
#    00 don't show any EMM's
#    01 show only valid EMM's, default setting
#    02 show valid and bad EMM's with complete data display
M: { 01 }

# ECM messages
#    00 don't show any ECM's
#    01 show only valid ECM's, default setting
#    02 show valid and bad ECM's with complete data display
C: { 01 }

# Emu
#    00 Card is running - gbox Emu is off (default)
#    01 Card is off - Emu is running
E: { 01 }

# Save Raw EMM
#    00 No raw EMM are saved  (default)
#    01 Raw EMM are saved in keyfile
#    02 Raw EMM and card commands are saved in keyfile
D: { 00 }

# AU
#    00 is ignored (default)
#    01 enable AU
#    01 AU Auto
A: { 01 }

# Emu for PW
#    00 Use Emu for PW(default)
#    01 Use Card for PW
P: { 00 }

# Key update
#    01 update only new keys, default setting
#    02 update all keys (used for valid PMK checking)
U: { 01 }

# Key files folder
#    00 keyfiles in /var/keys
#    01 keyfiles in /var/tmp
T: { 00 }

# # Hash pids
#    00 hash all pids
#    01 hash only pids with implemented algos (default)
H: { 01 }

# gbox Mode
#    00 Pure emu
#    01 Pure Softcam
#    02 pure Net Client
#    03 Mix Mode
G: { 03 }

# On Screen Display for Multicam 
#    00 No OSD (default)
#    01 display Smartcard messages, box IP required
#    02 display Smartcard messages new nhttpd format, box IP required
O: { 00 } 192.168.1.25    #OSD IP set by Enigma

# Init UDP Port
#    00 Off 
#    01 On
L: { 00 } 192.168.1.2 8017

Z: { 00 11 } 192.168.1.2  8020

V: { 00 10 }

J: { 03 02 02 01 01 }
F: { 01 } /tmp/pmt0.tmp          // pmt file
F: { 21 } /dev/demuxapi     // ca device
F: { 23 } /dev/demuxapi  // demux device
 