#Download from http://digsat.net
#Made by losten
# EMM messages
#    00 don't show any EMMs (default)
#    01 show only valid EMMs
#    02 show valid and bad EMMs with complete data display
M: { 01 }

# ECM messages
#    00 don't show any ECMs
#    01 show only valid ECMs (default)
#    02 show valid and bad ECMs with complete data display
C: { 01 }

# AU
#    01 enable AU
#    02 AU Auto
#    03 network cards update only
A: { 01 }

# key update (sum 01 or 02 with 04)
#    01 update only new keys, default setting
#    02 update all keys (used for valid PMK checking)
#    04 replace (not add) http-aes keys, only first key replaced !
U: { 01 }

# config files folder (softcam, autoroll, ignore/priority)
#    00 files in /var/keys
#    01 files in /tmp
T: { 00 }

# network mode, use summ for several clients
#    00 no network (default)
#    01 newcamd netclient
#    02 radegast netclient
#    04 camd3 netclient
G: { 01 }

# network retry, use summ for several options
#    00 disable
#    01 retry every new ecm
#    02 try to connect to offline shares every Q: seconds
#    04 try to detect and fast reconnect to lost (and not used atm) server
N: { 07 }

# network ecm timeout in seconds
K: { 10 }

# newcamd dead routes connect retry, sec
Q: { 600 }

# network shares priority
# 00 newcamd, radegast, camd3 (default)
# 01 camd3, radegast, newcamd
# 02 newcamd, camd3, radegast
P: { 00 }

# on screen display type
#    00 No OSD (default)
#    01 neutrino
#    02 enigma
#    03 relook
O: { 00 }

# on screen display Options, summ of:
#    01 show emu ecm 
#    02 show network shares messages
#    04 show decoding failed / fta
#    08 show emm keys update
S: { 03 }

# Log option, summ of:
#    00 Off
#    01 Network
#    02 console
#    04 file, appended ! delete it by yourself, before it eat all your hdd
L: { 00 } 

# keep ecm cache, seconds
E: { 15 }

# cache option, summ of:
#    00 Off (default)
#    01 Ecm pids cache, store pids used to decode in /tmp/ca_cache.list at exit, load at startup, same syntax as restore.list
#    02 Ecm data cache, remember CW for (E:) time 
#    04 Emm cache for network cards, do not resend the same emm twice, cache not cleared until restart
H: { 07 }

# reread files, summ of: 
#    00 No (default)
#    01 reread config file on channel change (including priority and ignore, but not replace/cache)
#    02 reread SoftCam.Key on channel change
#    04 reread SoftCam.Key if file changed
R: { 04 }

# debug, summ of
# 00 off (default)
# 01 debug ecm
# 02 debug emm
# 04 debug network ecm
# 08 debug network emm
# 16 debug network login
# 32 show mem/cpu stats every 1 min
# 64 add timestamp to log messages
D: { 00 }

# box type
# 00 autodetect, change only if you think wrong type detected.
# 01 dbox2
# 02 dreambox
# 03 triple-dragon
# 04 relook
# 05 openbox
B: { 00 }


# urls for aes keys update, any number or urls allowed,
# url data must contain key in format 0500:007C00:0000000000:00:key1:keyl
W: { http://some.host.com/keys.php }
