  relook300s software release

  released version  : 4.0
  released date     : Fri Apr 14 11:05:19 KST 2006
  released by       : porori

	1. Version 

    - boot loader
      U-Boot 1.1.1 (Apr 14 2006 - 17:15:09)
    - application
      4.0


  2. released files

    - README
    readme file.
    - serial_all_noboot.img
    via serial port, it updates all without u-boot.
    - serial_kernel_root_db.img
    via serial port, it updates linux kernel, application, db.
    it requires rescanning of channels.
    - serial_kernel_root.img
    via serial port, it updates linux kernel, application.
    - serial_uboot.img
    via serial port, it updates boot loader.
    - usb_all_noboot.img
    via usb port, it updates all without u-boot.
    - usb_kernel_root.img
    via usb port, it updates linux kernel, application.
    - usb_kernel_root_db.img
    via usb port, linux kernel, application, db.
    it requires rescanning of channels.
    - usb_uboot.img
    via usb port, it updates boot loader.


  3. How to download

    -Check your current program version first: 
      * Main menu-->About-->system info -->program version.
      * If the boot version is older than its newly released, 
      uboot.img has to be downloaded.
      * If the program version is older than its newly released, 
      all_noboot.img has to be downloaded.

  4. Known Bug

    -


  5. Changes

    - 4.0
      * EPG menu UI.Modified.
      * Record plan list was displayed unperperly. Bug Fixed.
      * Bug causing wrong display in each language on EPG : Bug Fixed   
      * Long length EPG is displayable at once : Function Added.   
      * When EPG program changes, time shift buffer become reset.Bug fixed.
      * EPG list is available on live banner: Function Added.
      * Subtitle and teletext is recordable: Function Added. 
      * Recording time options change each time the record button is
      pressed(RCU) on Live banner. Function Added.
      * When recording starts, new option is available whether the stored 
      content in time shift buffer or not: Function Added.
      * Reserved recording starts automatically when it is reserved 
      on second tuner: Function Added. 
      * Time shift buffer length is selectable: Function Added.  
      * Book mark fucntion was not working during the file play mode.Bug fixed.
      * Imputing special charactors are prevented as a file names: Function Added.
      * When channle search is complete, channels from the last TP scanned
      will be displayed. Function Added.
      * Leceiving local time data from satellites is enabled: Function Added.
      * Channel list structure is modified.New
      * Channel lists can be sorted by provider: Function Added.
      * In most UI meun page, Left/Down buttons perform as same function as
      the  page Up/Down buttons. Function Added.
      * DB : Updated 
      * Fan control options(Auto/On/Off) are available now. : Funtion Added  
      * LNB Setting is available on Diseqc 1.2/USALS menu: Function Added. 
      * Radio background image is changed: New
      * via serial cable, file down/up load possible.: New
      * allow to users to select diseqc from 1.1 to 16 switches: changed

    - 3.0.0 Changes
      * Time shift on/off is selectable in main menu: Function Added.
      * Default recording time options are selectable in main mene page:  Function Added.
      * When channel is switched or file is played on channel list or cms list, 
      those window don't disappear unless the OK button(RCU) is pressed twice.  :Function Added.

    -2.9.0 Changes
      * When recorded files are uploaded via usb, some special charactor
        appears infront of file name which prevents expoting the files.Bug Fixed.
      * When some channels(ex: premiere channels) are discrambled by CAM, AC3 
        did not work. Bug fixed.
      * Slovak , Czech and Hungarian are added to OSD language.: Added
      * Slovak , Czech and Hungarian are added to Default audio and subtitle  language.: Added 

    -2.8.0 Changes
      * USB file transfer did not function properly in previous 2.7 version: Bug fixed.

    -2.7.0 changes
      * Time zone OSD string : Modified.

    -2.6.0 Changes
      * Malfunction appears when the up/down keys are pushed and held 
      for long time. : Bug Fixed 
      * Showing wrong channel numbers in several menus after using channel 
      reordering function. Bug Fixed.

    -2.5.0 Changes
      *xcrypt smart card is supported.: Function Added. 

    -2.4.0 Changes
      * Firecrypt smart card is supported.: Funciton Added. 
      * When channels are scanned ,TV/Radio channels were not sorted 
      properly: Bug Fixed.
      * Blank appears when a new EPG program starts. Bug fixed. 
      * Bug which is causing the reset on time shift buffer when a new EPG 
      program starts.: Bug Fixed. 
      * EPG detail description lines are extended from 5 lines to 7 lines: Function added.
      * Displaying full long channel names on top left is enabled. Function Added.  
   
    -2.3.0  Changes
      * Two channels can be descrambled with one smart card simultanously.:
      Function Added.
      * If channel is switched right after trick-play, pixelation appears:Bug fixed
      * When trick-play such as jump, ramdom play, picture displays as a 
      blank page.:Function Added. 

    -2.2.8 Changes
      * Aston and matrix CAM can't descramble in several channels. : Bug Fixed 
      * Descrambles two channels simultaneously with one viaccess CAM.: Function Added. 
      * Blinking problem on info-message window.: Problem Fixed.

    -2.2.7 Changes
      * When file transfer is executed in USB mode, PANIC occurs.: Bug Fixed.
      * When Slow motion 1/2 is played, picture is broken or abnormal.: Bug Fixed.

    -2.2.6 Changes
      * STB stops functioning in several viaccess encrypted channels.: Bug Fixed 

    -2.2.5 Changes
      * While STB is working, unpluging the power code forcibly causes PANIC
      accompanying broken database. Bug Fixed.
      * Descrambling channels is not working in several viaccess channels 
      with Viacess CAM. : Bug Fixed 

    -2.2.4 Changes
      * Several cams ( ex.neotion zeta cam, premium x cam) are not decoded 
      or descrambled.: Fixed 
      * Several cams (ex. dragon cam ) can not be recognized when they are 
      inserted. Decording is not working either.:Bug Fixed
      * If warm boot is performed while CAM is inserted and left inside, 
      PANIC occurs rarely. : Bug Fixed. 
      * When screen is set 16:9 in 4:3LB mode, green line dispalys on the 
      picture: Bug fixed.
      * Indicating wrong Left / Right selectable value in alternate audio 
      menu.: Bug Fixed.
      * Radio and TV channels are not sorted the way it supposed to : Bug Fixed.
      * When Info button is pressed in channle list, channel PID dispalys as 
      8191.: Bug Fixed.
      *  Pixelation appears on UI in EPG menu.: Bug Fixed. 
      *  Without mounting a HDD, rerely STB stops functioning while channel 
      change.: Bug fixed.

    -2.2.3 Changes
      * When several cards left inside the STB, after while STB stops
        functiong : Bug Fixed. 
      * After using PC editor, STB rarely stops functioning.: Bug Fixed.
     
    -2.2.2 Changes
      * Right after channel search, if the power code is unpluged forcibly, 
      the searched data won't be stored: This is mostly happens on STB 
      without HDD: Bug fixed.
      * When Diseqc 1.2 is used, postion storing function does not work on 
      serveral satellites.: Bug fixed.

    -2.2.1 Changes
      * When channel list is on, "Panic" displays after deleting settings on 
      lnb setting menu.: Bug Fixed.
      * If there is channels without LNB settings, those channels displays as 
      "inactive" in channel list.

    -2.2.0 Changes
      * diseqc 1.1 : Supported 
      * Dutch langauage : Supported 
      * Channels search is sucessfully complete but it can not be stored 
      in DB.: Bug Fixed.
      * Recorded files from one STB can be copied to another STB' HDD which 
      enables to play the recorded files: Function Added.       
      * Picture appears as Black and white only in case of using old TV.: Bug Fixed      



  6. caution

    -

vim:set ts=2 sw=2 et tw=78 ai fileencoding=cp949 ff=dos:
